**Net 1060 Introduction to Networks Lab: # 10.4.4**

**Name: Andrew Koenig**

**Follow the instructions down below for the lab itself. For this lab, all answers need to be in blue font. For the questions right below, answer in complete sentences. Ensure you paste the screen shot of your score page at the bottom of the document. Even if this does not let you see your grade, still take a screen shot of the score page showing congratulations “your name” you have completed the exercise is pasted at the bottom of this document. You will then need to upload both this word document and your packet tracer file to the assignments link within Netacad. Let the instructor know if you have any questions.**

***Lab Analysis Report***

1. Using complete sentences summarize work you completed during the lab.

I set up a switch and router and configured a small network

2. Using complete sentences describe what you learned from the lab. Hint; look at the lab objectives listed at the top of the lab section.

I learned further how to configure a router and switch on a network.

***Problems Encountered***

1. Using complete sentences describe any problem(s) experienced during lab.

No problems

2. Using complete sentences describe how you solved your problem(s).

No problems

3. Using complete sentences explain if you needed any assistance with the lab; then list what you learned from that assistance. No problems

Packet Tracer - Build a Switch and Router Network - Physical Mode

# Topology



# Addressing Table

| Device | Interface | IP Address / Prefix | Default Gateway |
| --- | --- | --- | --- |
| R1 | G0/0/0 | 192.168.0.1 /24 | N/A |
| R1 | G0/0/0 | 2001:db8:acad::1/64 | N/A |
| R1 | G0/0/0 | fe80::1 | N/A |
| R1 | G0/0/1 | 192.168.1.1 /24 | N/A |
| R1 | G0/0/1 | 2001:db8:acad:1::1/64 | N/A |
| R1 | G0/0/1 | fe80::1 | N/A |
| S1 | VLAN 1 | 192.168.1.2 /24 | 192.168.1.1 |
| PC-A | NIC | 192.168.1.3 /24 | 192.168.1.1 |
| PC-A | NIC | 2001:db8:acad:1::3/64 | fe80::1 |
| PC-B | NIC | 192.168.0.3 /24 | 192.168.0.1 |
| PC-B | NIC | 2001:db8:acad::3/64 | fe80::1 |

Blank Line - no additional information

# Objectives

Part 1: Set Up the Topology

Part 2: Configure Devices and Verify Connectivity

Part 3: Display Device Information

# Background / Scenario

This is a comprehensive activity to review the IOS commands you have learned. In this Packet Tracer Physical Mode (PTPM) activity, you will cable the equipment as shown in the topology diagram. You will then configure the devices to match the addressing table. After the configurations have been saved, you will verify your configurations by testing for network connectivity.

After the devices have been configured and network connectivity has been verified, you will use IOS commands to retrieve information from the devices to answer questions about your network equipment.

This activity provides minimal assistance with the commands necessary to configure the router. Test your knowledge by trying to configure the devices without referring to the course content or the previous activities.

# Instructions

## Set Up the Topology

* + - 1. Move the required router and switch from the **Shelf** to the **Rack**.
      2. Move the required PCs from the **Shelf** to the **Table**.
      3. Cable the devices, as shown in the **Topology** and the **Addressing Table**.
      4. Power on all the devices.

## Configure Devices and Verify Connectivity

In this part, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords. Refer to the **Topology** and **Addressing Table** at the beginning of this activity for device names and address information.

### Assign static IP information to the PC interfaces.

* + - 1. On PC-A, configure the IP address, subnet mask, and default gateway settings.
      2. On PC-B, configure the IP address, subnet mask, and default gateway settings.
      3. From a command prompt window on PC-A, ping PC-B.

#### Question:

Why were the pings not successful?

Type yourI haven’t configured the devices yet. answers here.

### Configure the router.

* + - 1. Console into the router and enable privileged EXEC mode.

Open configuration window

* + - 1. Enter configuration mode.
      2. Assign the device name to the router.
      3. Assign **class** as the privileged EXEC encrypted password.
      4. Assign **cisco** as the console password and enable login.
      5. Assign **cisco** as the vty password and enable login.
      6. Encrypt the plaintext passwords.
      7. Create a banner that warns anyone accessing the device that unauthorized access is prohibited.
      8. Configure and activate both interfaces on the router.
      9. Configure an interface description for each interface indicating which device is connected to it.
      10. To enable IPv6 routing, enter the **ipv6 unicast-routing** command.
      11. Save the running configuration to the startup configuration file.
      12. Set the clock on the router.

**Note**: Use the question mark (**?**) to help with the correct sequence of parameters needed to execute this command.

Close configuration window

* + - 1. From a command prompt window on PC-A, ping PC-B.

**Note**: If pings are not successful, the Windows Firewall may need to be turned off.

#### Question:

Were the pings successful? Explain. Yes, the devices are configured now so traffic should be able to be routed.

Type your answers here.

### Configure the switch.

In this step, you will configure the hostname, the VLAN 1 interface, and its default gateway.

Open configuration window

* + - 1. Console into the switch and enable privileged EXEC mode.
      2. Enter configuration mode.
      3. Assign a device name to the switch.
      4. Configure and activate the VLAN interface on the switch S1.
      5. Configure the default gateway for the switch S1.
      6. Save the running configuration to the startup configuration file.

### Verify connectivity end-to-end connectivity.

* + - 1. From PC-A, ping PC-B.
      2. From S1, ping PC-B.

All the pings should be successful.

Close configuration window

## Display Device Information

In Part 3, you will use **show** commands to retrieve interface and routing information from the router and switch.

### Display the routing table on the router.

* + - 1. Use the **show ip route** command on R1 to answer the following questions.

Open configuration window

#### Questions:

What code is used in the routing table to indicate a directly connected network?

Type your C here.

How many route entries are coded with a C code in the routing table?

Type your 2 here.

What interface types are associated to the C coded routes?

Type your G0/0/0 and G0/0/1 here.

* + - 1. Use the **show ipv6 route** command on R1 to display the IPv6 routes.

### Display interface information on R1.

* + - 1. Use the **show interface g0/0/1** to answer the following questions.

#### Questions:

What is the operational status of the G0/0/1 interface?

Type your port is up and line protocol is up here.

What is the Media Access Control (MAC) address of the G0/1 interface?

Type your 0060.4731.8102 here.

How is the internet address displayed in this command?

Type your answers 192.168.1.1/24.

* + - 1. For the IPv6 information, enter the **show ipv6 interface *interface*** command.

### Display a summary list of the interfaces on the router and switch.

There are several commands that can be used to verify an interface configuration. One of the most useful is the **show ip interface brief** command. The command output displays a summary list of the interfaces on the device and provides immediate feedback about the status of each interface.

* + - 1. Enter the **show ip interface brief** command on R1.

R1# **show ip interface brief**

* + - 1. Enter the **show ipv6 interface brief** command on R1 to see the IPv6 interface information.

R1# **show ipv6 interface brief**

Close configuration window

* + - 1. Enter the **show ip interface brief** command on S1.

Open configuration window

S1# **show ip interface brief**

Close configuration window

# Reflection Questions

* 1. If the G0/0/1 interface showed that it was administratively down, what interface configuration command would you use to bring the interface up? No shutdown

Type your answers here.

* 1. What would happen if you had incorrectly configured interface G0/0/1 on the router with an IP address of 192.168.1.2? The computers would not be able to communicate because they would be on different networks.

Graphical user interface, application

Description automatically generated

R1#show run

Building configuration...

Current configuration : 1179 bytes

!

version 15.4

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname R1

!

!

!

enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1

!

!

!

!

!

!

ip cef

ipv6 unicast-routing

!

no ipv6 cef

!

!

!

!

!

!

!

!

!

!

no ip domain-lookup

!

!

spanning-tree mode pvst

!

!

!

!

!

!

interface GigabitEthernet0/0/0

description first port

ip address 192.168.0.1 255.255.255.0

duplex auto

speed auto

ipv6 address FE80::1 link-local

ipv6 address 2001:DB8:ACAD::1/64

!

interface GigabitEthernet0/0/1

description second port

ip address 192.168.1.1 255.255.255.0

duplex auto

speed auto

ipv6 address FE80::1 link-local

ipv6 address 2001:DB8:ACAD:1::1/64

!

interface GigabitEthernet0/1/0

switchport mode access

!

interface GigabitEthernet0/1/1

switchport mode access

!

interface GigabitEthernet0/1/2

switchport mode access

!

interface GigabitEthernet0/1/3

switchport mode access

!

interface Vlan1

no ip address

shutdown

!

ip classless

!

ip flow-export version 9

!

!

!

banner motd ^CAuthorized Users Only!^C

!

!

!

!

line con 0

password 7 0822455D0A16

login

!

line aux 0

!

line vty 0 4

password 7 0822455D0A16

login

!

!

!

End

S1#show run

Building configuration...

Current configuration : 1148 bytes

!

version 15.0

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname S1

!

!

!

!

no ip domain-lookup

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

ip address 192.168.1.2 255.255.255.0

!

ip default-gateway 192.168.1.1

!

!

!

!

!

!

line con 0

!

line vty 0 4

login

line vty 5 15

login

!

!

!

!

end