**Net 1060 Introduction to Networks Lab: # 7.3.7**

**Name:**

**Follow the instructions down below for the lab itself. For this lab, all answers need to be in blue font. For the questions right below, answer in complete sentences. You will also have to copy and paste your running configurations of each device configured to the bottom of this document. Let the instructor know if you have any questions.**

***Lab Analysis Report***

1. Using complete sentences summarize work you completed during the lab.

I made a small network, configured the devices, and learned how mac addresses get recorded

2. Using complete sentences describe what you learned from the lab. Hint; look at the lab objectives listed at the top of the lab section.

I learned how devices record device mac addresses

***Problems Encountered***

1. Using complete sentences describe any problem(s) experienced during lab.

No problems

2. Using complete sentences describe how you solved your problem(s).

No problems

3. Using complete sentences explain if you needed any assistance with the lab; then list what you learned from that assistance.

No problems

**Lab - View the Switch MAC Address Table**

# Topology



# Addressing Table

| Device | Interface | IP Address | Subnet Mask |
| --- | --- | --- | --- |
| S1 | VLAN 1 | 192.168.1.11 | 255.255.255.0 |
| S2 | VLAN 1 | 192.168.1.12 | 255.255.255.0 |
| PC-A | NIC | 192.168.1.1 | 255.255.255.0 |
| PC-B | NIC | 192.168.1.2 | 255.255.255.0 |

# Objectives

Part 1: Build and Configure the Network

Part 2: Examine the Switch MAC Address Table

# Background / Scenario

The purpose of a Layer 2 LAN switch is to deliver Ethernet frames to host devices on the local network. The switch records host MAC addresses that are visible on the network, and maps those MAC addresses to its own Ethernet switch ports. This process is called building the MAC address table. When a switch receives a frame from a PC, it examines the frame’s source and destination MAC addresses. The source MAC address is recorded and mapped to the switch port from which it arrived. Then the destination MAC address is looked up in the MAC address table. If the destination MAC address is a known address, then the frame is forwarded out of the corresponding switch port associated with that MAC address. If the MAC address is unknown, then the frame is broadcasted out of all switch ports, except the one from which it came. It is important to observe and understand the function of a switch and how it delivers data on the network. The way a switch operates has implications for network administrators whose job it is to ensure secure and consistent network communication.

Switches are used to interconnect and deliver information to computers on local area networks. Switches deliver Ethernet frames to host devices identified by network interface card MAC addresses.

In Part 1, you will build a multi-switch topology with a trunk linking the two switches. In Part 2, you will ping various devices and observe how the two switches build their MAC address tables.

**Note**: The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.2(2) (lanbasek9 image). Other switches and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and output produced might vary from what is shown in the labs.

**Note**: Make sure that the switches have been erased and have no startup configurations. If you are unsure contact your instructor.

# Required Resources

* 2 Switches (Cisco 2960 with Cisco IOS Release 15.2(2) lanbasek9 image or comparable)
* 2 PCs (Windows with terminal emulation program, such as Tera Term)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet cables as shown in the topology

**Note**: The Fast Ethernet interfaces on Cisco 2960 switches are autosensing and an Ethernet straight-through cable may be used between switches S1 and S2. If using another model Cisco switch, it may be necessary to use an Ethernet crossover cable.

# Instructions

## Build and Configure the Network

### Cable the network according to the topology.

### Configure PC hosts.

### Initialize and reload switches as necessary.

### Configure basic settings for each switch.

Open configuration window

* + - 1. Configure device name as shown in the topology.
      2. Configure IP address as listed in Addressing Table.
      3. Assign **cisco** as the console and vty passwords.
      4. Assign **class** as the privileged EXEC password.

Close configuration window

## Examine the Switch MAC Address Table

A switch learns MAC addresses and builds the MAC address table, as network devices initiate communication on the network.

### Record network device MAC addresses.

* + - 1. Open a command prompt on PC-A and PC-B and type **ipconfig /all**.

Open Windows command prompt

#### Question:

What are the Ethernet adapter physical addresses?

PC-A MAC Address:

Type 0004.9AB4.E93B answers here.

PC-B MAC Address:

Type 0060.5C76.5190 answers here.

Close Windows command prompt

* + - 1. Console into switch S1 and S2 and type the **show interface F0/1** command on each switch.

Open a configuration window

#### Questions:

On the second line of command output, what is the hardware addresses (or burned-in address [bia])?

S1 Fast Ethernet 0/1 MAC Address:

Type 0001.6455.a101 answers here.

S2 Fast Ethernet 0/1 MAC Address:

Type 0060.4748.4c01 answers here.

Close a configuration window

### Display the switch MAC address table.

Console into switch S2 and view the MAC address table, both before and after running network communication tests with ping.

* + - 1. Establish a console connection to S2 and enter privileged EXEC mode.

Open a configuration window

* + - 1. In privileged EXEC mode, type the **show mac address-table** command and press Enter.

S2# **show mac address-table**

Even though there has been no network communication initiated across the network (i.e., no use of ping), it is possible that the switch has learned MAC addresses from its connection to the PC and the other switch.

#### Questions:

Are there any MAC addresses recorded in the MAC address table?

Type your answers hereYes

What MAC addresses are recorded in the table? To which switch ports are they mapped and to which devices do they belong? Ignore MAC addresses that are mapped to the CPU.

Type your answers here. 0001.6455.a101

If you had not previously recorded MAC addresses of network devices in Step 1, how could you tell which devices the MAC addresses belong to, using only the output from the **show mac address-table** command? Does it work in all scenarios?

Type your answers here.It shows the port that the address is connected to, probably not all the time.

### Clear the S2 MAC address table and display the MAC address table again.

* + - 1. In privileged EXEC mode, type the **clear mac address-table dynamic** command and press **Enter**.

S2# **clear mac address-table dynamic**

* + - 1. Quickly type the **show mac address-table** command again.

#### Questions:

Does the MAC address table have any addresses in it for VLAN 1? Are there other MAC addresses listed? There are none listed now

Type your answers here.

Wait 10 seconds, type the **show mac address-table** command, and press Enter. Are there new addresses in the MAC address table? Yes the same one popped up again

Type your answers here.

Close a configuration window

### From PC-B, ping the devices on the network and observe the switch MAC address table.

* + - 1. From PC-B, open a command prompt and type **arp -a**.

Open a command prompt

#### Question:

Not including multicast or broadcast addresses, how many device IP-to-MAC address pairs have been learned by ARP? None

Type your answers here.

* + - 1. From the PC-B command prompt, ping PC-A, S1, and S2.

#### Question:

Did all devices have successful replies? If not, check your cabling and IP configurations.

Type Yes all devices had successful pings answers here.

Close a command prompt

* + - 1. From a console connection to S2, enter the **show mac address-table** command.

Open a configuration window

#### Question:

Has the switch added additional MAC addresses to the MAC address table? If so, which addresses and devices? Yes there are 4 devices now, all of the devices on the network

0001.6455.a101

0004.9ab.e93b

00060.5c75.5190

00d0.d3ed.196a

Type your answers here.

Close a configuration window

Open a command prompt

From PC-B, open a command prompt and retype **arp -a**.

#### Question:

Does the PC-B ARP cache have additional entries for all network devices that were sent pings?

Yes, it has all the other devices on the network. your answers here.

Close a command prompt

# Reflection Question

On Ethernet networks, data is delivered to devices by their MAC addresses. For this to happen, switches and PCs dynamically build ARP caches and MAC address tables. With only a few computers on the network this process seems fairly easy. What might be some of the challenges on larger networks? With so many devices you could have extra signals bouncing around until they find a device with the needed address of the destination which is unnecessary.

Type your answers here.

Diagram

Description automatically generated

S1#show run

Building configuration...

Current configuration : 1194 bytes

!

version 15.0

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname S1

!

enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1

!

!

!

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

ip address 192.168.1.11 255.255.255.0

!

!

!

!

line con 0

password cisco

login

!

line vty 0 4

password cisco

login

line vty 5 15

password cisco

login

!

!

!

!

End

S2#show run

Building configuration...

Current configuration : 1194 bytes

!

version 15.0

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname S2

!

enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1

!

!

!

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

ip address 192.168.1.12 255.255.255.0

!

!

!

!

line con 0

password cisco

login

!

line vty 0 4

password cisco

login

line vty 5 15

password cisco

login

!

!

!

!

end